# Slot 3 Menu 2 − EoE Status

Mode: Open‑Loop

Ethernet over EtherCAT (EoE) Status.

Parameter | 3.02.003 EoE Status
--- | ---
Short description | Status of EoE
Minimum | 0 | Maximum | 6
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background Write
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT, BU

Value | Text | Description
0 | Initialising | The EoE interface is being initialised
1 | Link Down | No EoE connection has been detected
2 | Not Applicable |
3 | Not Applicable |
4 | Ready | The EoE interface has been successfully configured but no data is being received or transmitted
5 | Active | The EoE interface is receiving or transmitting data
6 | Active With Errs | The EoE interface is receiving or transmitting data but Receive errors have been detected

This is the status of the EoE interface

Parameter | 3.02.004 EoE Network Message Count
--- | ---
Short description | EoE Network Message Count
Minimum | 0.0 | Maximum | 6553.5
Default |  | Units | Messages/s
Type | 16 Bit Volatile | Update Rate | Background Write
Display Format | Standard | Decimal Places | 1
Coding | RO, ND, NC, PT, BU

This is the Average number of Ethernet frames received and transmitted via EoE

Parameter | 3.02.006 EoE IP Address
--- | ---
Short description | Shows the IP address of the module set by EoE
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | On EtherCAT initialisation
Display Format | IP Address | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Displays the IP address of the module, as set by Ethernet over EtherCAT (EoE).

Parameter | 3.02.007 EoE Subnet Mask
--- | ---
Short description | Shows the subnet mask of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | On EtherCAT initialisation.
Display Format | IP Address | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Displays the subnet mask of the module, as set by EoE.

Parameter | 3.02.008 EoE Default Gateway
--- | ---
Short description | Shows the default gateway of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate |
Display Format | IP Address | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Displays the default gateway of the module, as set by EoE.

Parameter | 3.02.011 EoE Virtual MAC Address
--- | ---
Short description | Shows the virtual MAC address of the module (as set by EoE)
Minimum | 0 (Display: 00:00:00:00:00:00) | Maximum | 281474976710655 (Display: FF:FF:FF:FF:FF:FF)
Default |  | Units |
Type | 64 Bit Volatile | Update Rate | On EtherCAT initialisation
Display Format | MAC Address | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Displays the MAC address for the EoE virtual Ethernet interface as a 48 bit hexadecimal value. For example “0A1C0034AB0C”.