Introdcution:

This release note is intended for using the simulator app only in the VLT Software Customizer plug-in which is a part of MCT-10 V4.00


Usage Instructions

The simulator files will have the below syntax and the externsion of the file being .zip (compressed format)

<Drive Model><Firmware Version>Simulator.zip

example: FC-102 05.02 Simulator.zip

The user is asked not to un-compress the .zip file, any action related to uncompression and usage of executables will not lead to any specifc functionality thereafter.

Step 1: Launch the MCT10 V4.00 Build 3770 and any higer version
Step 2: If you have created a new drive (or) imported online project which supports the new control card then the VLT Softwar Customizer plug-in shall be visible in the project tree
Step 3: Click 'Tools' in the menu and select 'Update VLT Software Customizer Support...'
Step 4: Select the respective file based on the type of project created (based on the drive model & Software version)
        You could easily know the drive model & software version which is the file name
Step 5: once "Open" button is clicked then the .zip file will load the simulator app to the MCT10 installation directory
Step 6: The app is now ready for simulatoting the configuration you have performed through the tool

If you still need assistance please contact Danfoss Representative.

